###### Using a Joystick as a Mouse

This script converts a joystick into a three-button mouse. It allows each button to drag just like a mouse button and it uses virtually no CPU time. Also, it will move the cursor faster depending on how far you push the joystick from center. You can personalize various settings at the top of the script.

Download This Script | Other Sample Scripts | Home

    ; Increase the following value to make the mouse cursor move faster:
    JoyMultiplier = 0.30

    ; Decrease the following value to require less joystick displacement-from-center
    ; to start moving the mouse.  However, you may need to calibrate your joystick
    ; -- ensuring it's properly centered -- to avoid cursor drift. A perfectly tight
    ; and centered joystick could use a value of 1:
    JoyThreshold = 3

    ; Change the following to true to invert the Y-axis, which causes the mouse to
    ; move vertically in the direction opposite the stick:
    InvertYAxis := false

    ; Change these values to use joystick button numbers other than 1, 2, and 3 for
    ; the left, right, and middle mouse buttons.  Available numbers are 1 through 32.
    ; Use the Joystick Test Script to find out your joystick's numbers more easily.
    ButtonLeft = 1
    ButtonRight = 2
    ButtonMiddle = 3

    ; If your joystick has a POV control, you can use it as a mouse wheel.  The
    ; following value is the number of milliseconds between turns of the wheel.
    ; Decrease it to have the wheel turn faster:
    WheelDelay = 250

    ; If your system has more than one joystick, increase this value to use a joystick
    ; other than the first:
    JoystickNumber = 1

    ; END OF CONFIG SECTION -- Don't change anything below this point unless you want
    ; to alter the basic nature of the script.

    #SingleInstance

    JoystickPrefix = %JoystickNumber%Joy
    Hotkey, %JoystickPrefix%%ButtonLeft%, ButtonLeft
    Hotkey, %JoystickPrefix%%ButtonRight%, ButtonRight
    Hotkey, %JoystickPrefix%%ButtonMiddle%, ButtonMiddle

    ; Calculate the axis displacements that are needed to start moving the cursor:
    JoyThresholdUpper := 50 + JoyThreshold
    JoyThresholdLower := 50 - JoyThreshold
    if InvertYAxis
        YAxisMultiplier = -1
    else
        YAxisMultiplier = 1

    SetTimer, WatchJoystick, 10  ; Monitor the movement of the joystick.

    GetKeyState, JoyInfo, %JoystickNumber%JoyInfo
    IfInString, JoyInfo, P  ; Joystick has POV control, so use it as a mouse wheel.
        SetTimer, MouseWheel, %WheelDelay%

    return  ; End of auto-execute section.

    ; The subroutines below do not use KeyWait because that would sometimes trap the
    ; WatchJoystick quasi-thread beneath the wait-for-button-up thread, which would
    ; effectively prevent mouse-dragging with the joystick.

    ButtonLeft:
    SetMouseDelay, -1  ; Makes movement smoother.
    MouseClick, left,,, 1, 0, D  ; Hold down the left mouse button.
    SetTimer, WaitForLeftButtonUp, 10
    return

    ButtonRight:
    SetMouseDelay, -1  ; Makes movement smoother.
    MouseClick, right,,, 1, 0, D  ; Hold down the right mouse button.
    SetTimer, WaitForRightButtonUp, 10
    return

    ButtonMiddle:
    SetMouseDelay, -1  ; Makes movement smoother.
    MouseClick, middle,,, 1, 0, D  ; Hold down the right mouse button.
    SetTimer, WaitForMiddleButtonUp, 10
    return

    WaitForLeftButtonUp:
    if GetKeyState(JoystickPrefix . ButtonLeft)
        return  ; The button is still, down, so keep waiting.
    ; Otherwise, the button has been released.
    SetTimer, WaitForLeftButtonUp, off
    SetMouseDelay, -1  ; Makes movement smoother.
    MouseClick, left,,, 1, 0, U  ; Release the mouse button.
    return

    WaitForRightButtonUp:
    if GetKeyState(JoystickPrefix . ButtonRight)
        return  ; The button is still, down, so keep waiting.
    ; Otherwise, the button has been released.
    SetTimer, WaitForRightButtonUp, off
    MouseClick, right,,, 1, 0, U  ; Release the mouse button.
    return

    WaitForMiddleButtonUp:
    if GetKeyState(JoystickPrefix . ButtonMiddle)
        return  ; The button is still, down, so keep waiting.
    ; Otherwise, the button has been released.
    SetTimer, WaitForMiddleButtonUp, off
    MouseClick, middle,,, 1, 0, U  ; Release the mouse button.
    return

    WatchJoystick:
    MouseNeedsToBeMoved := false  ; Set default.
    SetFormat, float, 03
    GetKeyState, joyx, %JoystickNumber%JoyX
    GetKeyState, joyy, %JoystickNumber%JoyY
    if joyx > %JoyThresholdUpper%
    {
        MouseNeedsToBeMoved := true
        DeltaX := joyx - JoyThresholdUpper
    }
    else if joyx < %JoyThresholdLower%
    {
        MouseNeedsToBeMoved := true
        DeltaX := joyx - JoyThresholdLower
    }
    else
        DeltaX = 0
    if joyy > %JoyThresholdUpper%
    {
        MouseNeedsToBeMoved := true
        DeltaY := joyy - JoyThresholdUpper
    }
    else if joyy < %JoyThresholdLower%
    {
        MouseNeedsToBeMoved := true
        DeltaY := joyy - JoyThresholdLower
    }
    else
        DeltaY = 0
    if MouseNeedsToBeMoved
    {
        SetMouseDelay, -1  ; Makes movement smoother.
        MouseMove, DeltaX * JoyMultiplier, DeltaY * JoyMultiplier * YAxisMultiplier, 0, R
    }
    return

    MouseWheel:
    GetKeyState, JoyPOV, %JoystickNumber%JoyPOV
    if JoyPOV = -1  ; No angle.
        return
    if (JoyPOV > 31500 or JoyPOV < 4500)  ; Forward
        Send {WheelUp}
    else if JoyPOV between 13500 and 22500  ; Back
        Send {WheelDown}
    return